Introduction

Railway terms and specific words must be used in the texts in the field of railway engineering.

These terms have been translated in Persian Academy (Farhangestan) since 1995.

The attachments are a number of railway terms and their equivalent Persian words including approved items in Farhangestan.

This file will be accordingly updated.

Should you have any query, do not hesitate to contact me.

Yours sincerely

Ali Asadi
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Interchange Station,
transfer,interchange
Junctionstation

Multi-level station

Intermodal station,
Multimodal station

Midblock stop

Degage
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Pallet

Overhaul

Wagon Weighbridge,
Freight CarScale,

Track Scale
WagonlLift,

Wagon Elevator

Credit Ticket

Reduced Fare Ticket

OneJourney Ticket

Full Fare Ticket

Fullday Ticket

Thorough Ticket

TicketDecoding Reading

Equipment, Ticket
Decoding Equipment

TicketValidation

Round Trip Ticket,
Return Ticket

FreeTicket

FullWay Ticket

Automatic Fare Collection
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Monthly Ticket

Season Ticket

Magnetic Ticket

Open Ticket

Weekly Ticket

Bogie, Truck

Self Steering Bogie

ThreePiece Bogie

BuffetCar

Rail Fastener, Fastener,

Rail Clip

Ballast

Monitoring
Rail Foot,Rail Base

Duty Pass

FreePass

Buttress

Buttressed

Gallery

Side-Tipping Wagon

People Mover
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Hump

IIZII bed

crossing,crossover

diamond crossing,

track crossing

double crossover,diamond
Crossover,SCiSsors Crossover,
universal crossover

grade separated crossing

interchange

level crossing,grade crossing,
highway-rail
gradecrossing

contactpatch

manoeuvre

marshalling yard,
shuntingyard

shunter

luggage,baggage

van

switchrail,tonquerail,
bladerail

railweb

locomotivecrane

inspection pit

examination-pit
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drop-pit

trolley

wheelset

trailingwheelset

flatwheel

wheelchair

trafficdensity

right-of-way

interlinetransportation

railfailure, rail defect

line

ballastregulator

track

continuous weldedtrack

trapsiding

draisine

siding,branchline
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dead-endsiding,
dead-endtrack

reversingtriangle

rolling stock

trainset

electricmultiple unit, EMU

diesel multiple unit, DMU

portion,serving

slabtrack

corridor

charter

stockrail joint
faregate

ticketvendingmachinegiving
change

accessibility

double heading,double engine

sightingdistance

demurrage

reservation
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generaltrackforeman

sectionforeman,
sectionboss

link

barrier

accesscorridor

ramp
rame

restaurantcar

rail

standardrail

wingrail,binderrail

rail saw

stationary rail saw

portable railsaw

make uprail, shortenedrail

couplage

longrail

traverse

stockrail

runningrail
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railbender

rail-grinding machine, rail
grindingtrain

lightrail

heavy rail

rail punch, rail drill
thirdrail,contactrail,current
collectorrail,

conductorrail
groovedrail,girderrail

rail stretcher,

rail pullingdevice

shortrail

rail heater

continuousweldedrail, CWR,
longweldedrail,weldedrail,
ribbonrail

guiderail,closurerail,leadrail

peakhours

underpass

slide chair

Railchair,chair

ticketbooking hall, ticket hall

running speed

express

contactpatch

crashworthiness
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Loading platform,goods platform

punch
switch, point
Catenary

turntable

ridingindextraffic

pantograph
traffic

ramp

loading ramp, slop of platform

grader

tampon

fleetcapacity

signalling
trunroundtime
servicelife

railflaw
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galley

restaurantcar

wheeltread

railtread

headway

wheelbase

freight

containertrain

monorail train,monorail

observationrailcar

turbotrain

tramway

ramereversible

lightrailtransit,LRT

ultra-low-floortram

funicularrailway

maglevtrain
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gabarit

loadinggauge

rerailing frog,humpback carfrog,
butterfly frog, wrecking frog,
greenback,rerailer

superelevation

curve marker
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rail mill
ferry-boatcoach

railhead, head ofrrail

coupe

check-inline

check-inline

exchange hall

rail lubricator

wheelflange

hybridlocomotive

dynamictrack stabilizer

rail welding machine

ballastregulator

ballastcompactor, ballast

consolidator

rail-grinding machine, rail

grindingtrain

track-laying machine
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ballasttamper,ballasttamping

machine

rail detector car,rail flaw detector

airfoil

track foreman

dwelltime

Route
Doubletrackline
Singletrackline

Assistanttrackforeman,
sub-foreman,leadman

Hostess

Steward,stewardess

Damping

Fleet,rolling stock

Base periodfleet

Foulingmark,
fouling point

track maintenance

Half-barrier

Wagon,car,vehicle

testwagon,testvehicle,

geometry car,evaluationcar

Ambulancewagon,

hospital car,ambulance coach
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tilting wagon, tilting coach

salooncoach

cattlewagon,stock car

freightwagon,freightcar,goods

wagon

steamwagon, heatingwagon
balastwagon,ballastcar
cranewagon,derrick car
caboose
sleepingwagon,sleeping car

car-carrierwagon

hopperwagon,hoppercar

high-floor car

low-floor car,low-floorwagon,
low-floorboarding

flatwagon,flatcar

compartmentcoach
highsidewagon
Lowsidewagon,gondolacar

tankwagon,tankcar
passengerwagon,
passengercar,car

Coveredwagon
covered car,boxcar

articulatedwagon

articulated coach
energy distributionwagon,

generatorwagon

Refrigeratorwagon, reefer
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wagonnet,smallwagon,spoit
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_1302784968.pdf
English terms, railway words

English Persian
Includes both the approved equivalent terms
and offered terms

Actuator 021 Jac ¢ Jlus 5y
AEA Technology Rail Ji 5858 ) )
Air bag ) sa i A4S
Aligning oS ) gna ad
Alignment i) yen
Alignment error il pea glad
Allowance 1) o S
Angle of attack alaa 4540
Arrangement
Articulated O Jaida
Articulated train (o3 Jada) jla Jiaia U
Asperity U paal
Assistant track foreman daali bl o glas
Attack 9 calas
Attack wheels oo sled a
Austenization O Al
Automatic fare collection Do A Ly b el
Axis 4l
Axle box (journal box) QUL 4ea
Axle spacing e aliald

Backstay cable

Balise ) S Cund e
Ball bearing Sy,
Beam element i ol
Beam link D5 il
Bearer Sl
Bearing gkl
Benchmarking s (o))
Bilinear vertical force Al 5w b adKsn Jad S35
Body FOVEN
Bogie offset Sis g s
Bounce S G (8 Oy 5 YL
Brake shoe RS
Buckling iilaS
Buffer stop (el e
Bumpstop DR 4 ] s Sasly
Calibration O sl s
Cant (DEVER) L2 ¢k
Cant deficiency 05 (mS ) 258
Cant excess BERUS
Cantrail Sl ol s
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Cartridge PR
Cast SRy
Catastrophic i
Centering SN0 pb
Centrebowl ERTTE S
Centrepivot 4 8 (5 S e a5 55 4wlS
Centreplate s (55 g0 4nlS
Chevron spring Gaosh i o Sk SGiuay i
Chord BT
Classification yard @ 2 ) 4ka gae
Clearance B slad - A (A
Coil spring (Fail) Jsb s
Coil sprung vehicles sl 4 jeae s (Kl
Compensation o) s
Component 4dl ga (L9 Canse 50) cdadal (o 10)
Configuration Sl ) e
Conformal JEFIEINY
Conformal contact e (ulad
Conicity Jabee o jia cuda g 3
Constant curving i ey s
Constraints 25
Contact surface ol s

Contour

u}i ot 40l col ald Lﬁ\.'\;.':\

Couple (in wheelset)

DSBS (o iz )

Constant <l
Contact area ol (Calise) mhass
Contact patch s&ilai ¢ el 4als
Contact stiffness ol Jids
Contour ke
Conventional o Hlia o glaia
Corrugate s
Counterbalanced Jalxtia

Contour

uﬂlﬁsu.ala"r\a.m' A ‘)}'.'\.'115

Couple (in wheelset)

OSAES iz )

Creep SR
Cross- level b aa X
Crossing (R ¢ sme o8&y 53) (5 ) i ()3 e el
Cross-section b
Curvature oo g lad (s
Curve s
Curving ey 8
Cut-in speed

Cylinder IS (o) Al gl
Damper R e co2ii€) 5
Damping )
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Dash pot BLHRERS
Datum plate (Uil alw) saly Cilaiin
Dead end siding oS ha
Debris b).J
Deflated A S
Deflection o
Derailment Li )z A
Derivation Y
Derivative ) atd
Detonator (Bad) 438 53
Diabolo profiles o=l Jd s
Dicone hsoae dis nbgled a
Differential Gl y3
Differentiation el
Dipped joints a8 iy o
Discretised ellipse (41l 02 arli (any
Disembark O ealy
Double heading SIS 5
Drop Sl cda gi
Drop pit Fads
Ductility oale LES Culid
Dynamic drop Sl ((Salidl) L giu
Dynamic lift Sl (VL) YL
Effective conicity Fise Cphag i
Eigen behavior Aadlae 8,
Eigenvalue o519 laia
Elastic limit i as
Elasticity =lad )l caduain)
Embark s ) s
Energy dissipation s 5 <)
Engine shed, locomotive shed 5 5a 581 LS
Envelope o)) g
Equation aday)  cdalaa
Equivalent cant 9 Jaa
Equivalent conicity Jolas a5 3
Examination pit a5k lla
Excitation o
Explicit resolution e s s
Exponential function (i adail
Expression aday) ) calalaa
Fabricate oK 5 s S Gy
Faces (S
Faint lines G bd (ay abals
Faregate & oa by (o3)5))
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Feedback D5 (A 90
Field e
Filtering GV Koy yils
First order Js) 4
Fishplate el Jlail 4siia
Flange 4l
Flanging clearance Jiy S Sl s adalale
Flange way clearance Ji) JUS 5 a il e A

Flange contact

iy DS L F o 4l Ll

Flat centre plate

G (55 5 AnlS

Flat wheel o L;.\g)g
Flaw(ed) A
Fore and aft RS
Fouling mark & el aSLES
Friction Sdaal
Friction pairs

Gauge Uae
Gauge side, gauge corner oy (43 5) o S
Gauge widening b e se gligy il 8
Gauging Syl g8
General track foreman aaliad i
Global reference frame & e Claida
Glued ballast st oYLy
Grain boundary S ),
Gravitational el R s
Hardness (i
Headcheck LS5 ) ik asus
High floor car YU < (Rl
Hollow wheel SR
Horn guide o)) g3 &
Housing S sh cdiug
Hum FUVINY
Hunting Sagiila
Hybrid S
Hyperbolic tangent Sl ulas
Hypothesis daa jb
Hystersis e [aile G
Impact 4 pia
Implicit PRI
Increment o
Incremental syl 3
Indentation contour @ 4l O & ay 4l
Individual RIS
Inertial i)
Inflated Ly
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Infringement

In-plane 38 Aadia
Intact et (o JalS
Integration $S
Interchange Jo g Jan dga yuas
Interchange station J8 5 Jan 20 s oK)
Interface Ui )
Interpenetration i 7 sl 3 g
Interpolated curve SO n e s
Intercepted contour OR (oan e 4l
Intermodal Calide slad g
Irregularity s saals
Journal selad (Jb g3
Journal bearing =l gl (all
Jump S
Jump width Jin sl
Kinematic envelope Silaia o )l 68
Lag als
Laser gauging vehicle G o) s Gamt alus g
Lasersweep Gusm ol
Leading S
Leading wheelset S e —F
Lead-lag

Leaf spring AT i (el
Linkage Ry
Loading soS b
Loading gauge S bol s
Loading platform oS b s S
Loading ramp SR b 4al ) cud
Local (A 5
Locked-in

Loop adls
Low-Bandwidth control Sl g J s
Lower-body ol o€ ol
Low floor car ol oS il /ol S (R
Lozening G (b 58l ¢ Sanls
Lubrication Gl
Main frame PR
Marshalling yard RCOWART
Mechanism OS5k
Meshing G e
Mild wear ol )l il
Misnomer (Fxe (2 Al
Modal properties I se Lal 62
Modal (structure) (e0w) JIase
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Mode shapes

LAJ}A(JS\.N

Modelling

Monitoring

by el ya

Monobloc wheel

Motion sickness

S a )l A g sl

Mounting oK 4S5l
Multi-body model (e dia Ja
Multiple contact Alaia ulad
Nested R Jal
Nominal play in the track hi pnails Jaadls
Non flanging Foa 4 Gl o5
Normal b 5 3see (Jlayi
Notional g
ORE (28 2l5) Lg ) L) s 3
Overthrow ST
Parabola JSE ags
Passive (o ES) Jlad e
Patch 4l
Pay load b
Pendulum linkage sk Juai
Periodical excitement o glita @l jag
Perturbation Uiline )
Pin pivot i eYsom
Pitch ae Aal e o) )50
Pivot Yl
Plain bearing (S8Ehal) il bl
Plank () Sl (and
Plate spring ek e
Positional Cuad ga
Possession o peat oS
Preload b Ui
Profile F i« Jdg
Projection’ (55) iy
Projection® AN
Pseudokinematic Soilaian 4ns
Pure Dicone sald ki ke
Push force L g5
Quadratic (s
Radially steered =i ol
Rail bar d...\) BB
Rail bender Seady
Rail detector car di b e ila
Rail failure BIEPEEN
Rail flaw Ji e

Last update: 4™ April 2009






Rail gauge oy (e 1S) 4i £
Rail heater Kol di)
Rail joint iy o
Rail lubricator For U pu K
Rail mill doy (25) Aa S
Rail punch S F s o
Rail saw »dy
Rail stretcher O day
Reference profile e s
Regression i ey s R
Relationship aday)  cadalae
Re-railing frog el
Residual Silawsy
Resonant EPEW
Ride quality/ Ride index BHENE
Rigid la
Rigid jump (et ) la alal G L) e iy
Roll Ao anl Joa o) 550
Roll/yaw gyroscope pld 5 (Job glysaaagl) Saes QS p
Roll bar o 4l
Roll drop

Roller Sale
Roller bearing Sy
Roller beam Sale
Roller rigs e Sl )l il e
Rolling idle
Rolling contact fatigue e Caaglia () 28L) Kiwa
Rolling force b Al Jsa S0 g0
Rolling stock )i (b adis Laila
Rotating L.J\)}J cu.'i;)e s 9 codid ja
Roughness za e (Hlals
Run-in @
Running gear S a4l )
Running rails S sla o)
Sampling S 4 sal
Saturation sy

Second order polynomials

psd 4a ) ) alenain

Section foreman dalad
Seizure S S
Self-excited Saadaa
Self-levelling system S 2 6A ailabl
Semi axis (U wan ) skl ey
Servo hydraulic suspension Slgoua 5y (Galat ailals
Settlement Cuniy
Severe wear 225 b

Shakedown limit

(aq})'é) TEPIVEIREN
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Shakeout

Shelling O (s) Al 5
Shimming SIX (ad) (Y
Shunting yard Jsile ada saa o dad) osl8iardais
Side wear ol il
Siding G LS baa
Single contact A Ll
Sky-Hook damping ) cla )y
Slab track ha Ja /g Jha
Slewing ring siA ya sl 4dla
Sliding oad i oad
Slip Al
Smooth friction oS Saial
Smoothing Skl se
Solebar

Solid s eala
Solid axle S saa
Solid wheel sl i gn 7 s
Spalling S
Spiral JI sl
Spring plank JEREERT
Sprung mass 22 (520 5 oy
Squats Ay
Squeal (&02) &=
Stability s olab
Stabilizing 221l
Stationary rail saw S di
Stepping distance OSL (51 5) Jual 58
Stiff spring Cabs i
Straight track aise Jad
Strain Ui S
Strain hardening NS
Stress ki
Structure gauge AL ) alay)

Strutting sleeper

il o gl il s (51 el a5l 53

Suspension

é.\u
-

Suspension swing

Sway ) o) 56S S8 A [ il (iad) Gl
Swept envelope s Jlad (sliab ¢ gal yu (slia
Swing BRSNS
Swing link s
Switch O3 s
Tache ovale & e paiadl
Tangent problem lae il
Tangent stiffness oles S
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Tangent track

e

Tensile strain SIS i S
Tension Jais
Theory ki ) 5
Throttle valve

Throw

Thrust O) 1 55
Tight curve 25y B
Tilting o g =S
Tilting trains (021 93 zS ) S5l b
Tolerance G gy il
Topography R
Torsion spring e
Toughness (e jia
Track La
Track alignment L il s
Track foreman La yila
Track frame i aa e oK
Track gauge Li e
Track irregularities Li 5 ) saals
Track panel (Wasly b sl 5 550 0 diy ) S ) 530S
Track twist o ba Saay
Traction Juis
Traction arm i€ e
Traction rod JasS 4l
Trailing (e
Trailing arm Lol Je /[ Gt (5530
Trailing wheelset SOH e —F
Transfer ha it oK)
Transient OIX
Transition X
Transition curve Sy L sh
Transition load Sy
Translational springs ) sla i
Trap siding omels Ja
Travel e ala
Tread (7 s2) 45k el
Trial Jiala
Trundle olile
Trundle speed

Turnout s ¢Sl
Twist Sy
Two axle 8 5493

Ultra low floor car

S LA uld (S 5 s

Ultra sonic flaw detection

sl Bl e

Universal

R e sae
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Universal mechanism

e Sk

Unsprung mass

(@i ye) Blaalia

Unstrained Al Aia
Vehicle gauge RSP
Vertical Al
Viscous damper z N oS e
Walkways s ey
Wayside La s
Wear Sl
Wedge S
Wheel plate (web, disc) For (Sew) ola
Wheel climb Eox (2sma) g, YL
Wheel flange Foarad
Wheel hub ST
Wheelset e -Fa
Wheel skid, wheel sliding Fox (Uiom) O
Wheel slip () e
Wheel squeal Fox i
Wheel surface & o> g
Wheel tread F o> o8l as sk
Wheel truing For )i s
Working shift SIS Cu g
Worn profile il Jad sy
Yaw Ald Al Jsa ol 50
Yield s
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